**Customer Connections – Policies**

EirGrid as TSO, plan, manage, develop and operate the national electricity transmission grid at 110, 220, 275 & 400kV across the island of Ireland, acting as a Transmission System Operator TSO.

EirGrid develops and maintains Transmission Investment Policies setting out the acceptable standards and regulations for Transmission developments.

Below is a non-exhaust list of policies that may be of interest to Customers seeking connections.

**Transmission Policy Documents**

|  |  |
| --- | --- |
| **No.** | **Drawing Title** |
| **1** | Access to TSO Current and Voltage Instrument Transformer Cores |
| **2** | Policy on Wind Turbine Clearance to OHL’s |
| **3** | Policy on Calculation of the Maximum Fault Level for Substation Earth Grid Design |
| **4** | Policy Statement on Busbar Configuration for 110, 220 and 400 kV Transmission Substations |

**Customer Connections – Standards**

EirGrid maintains and develops drawings and technical standards and functional specifications for connections to the Irish Transmission System. These standards govern the design and construction of new transmission assets namely Transmission substations, cables and overhead line feeder circuits.

Below is a non-exhaustive list of commonly used technical standards on 110 kV and 220 kV Transmission connections for demand and generation customer’s to consider when developing their connection projects and associated planning applications.

**Technical standards information on Transmission grid connections**

|  |  |  |
| --- | --- | --- |
| **No.** | **Drawing Title** | **Drawing Number** |
| 1 | Customer 110kV AIS C-Type SLD | XDN-SLD-STND-005-R02 |
| 2 | Customer 110kV GIS C-Type SLD | XDN-SLD-STND-H-006-R01 |
| 3 | 110kV AIS Loop Station – Initial C-shape build layout | XDN-LAY-ELV-STND-H-001-R07 |
| 4 | 110kV AIS Single Transformer Tail Station | XDN-LAY-ELV-STND-H-003 |
| 5 | 110 kV Single Bay Extendable to C-type station | XDN-LAY-ELV-STND-H-006 |
| 6 | 110kV AIS Station Typical Control Room Layout | XDN-CR-STND-H-001-R01 |
| 7 | 110 kV GIS Station Layout (8 Bay) | XDN-LAY-ELV-STND-H-012-R0 |
| 8 | [Transmission Line and Solar Farm Guideline Clearances](https://buzz.grid.ie/sites/GridDevelopment/tem/drawing_library/Approved%20Drawings/IPP%20Drawing%20Pack/Solar%20Farm%20Guideline%20Clearance%20Drawings%20-%20Jan%202019/Transmission%20Line%20and%20Solar%20Farm%20Guideline%20Clearances.pdf) | MMD-373966-E-SK-XX-11, 12, 12, 21, 22, 23 |
| 9 | 110/220/400kV Station General Requirements | XDS-GFS-00-001-R4 |
| 10 | 110 kV Underground Cable Functional Specifications | CDS-HFS-00-001 |

**Recently Published Standards in 2019**

|  |  |  |  |
| --- | --- | --- | --- |
| **No.** | **Document Title** | **Document Number** | **Revision Date** |
| 1 | GIS Functional Specification | XDS-GFS-25-001-R4 | 21/01/2019 |
| 2 | 110 kV Single Bay Extendable to C-type station | XDN-LAY-ELV-STND-H-006-R0 | 13/02/2019 |
| 3 | 110 kV GIS Station Layout (8 Bay) | XDN-LAY-ELV-STND-H-012-R0 | 26/09/2019 |
| 4 | 110kV AIS Single Transformer Bay Tail Station Layout | XDN-LAY-ELV-STND-H-003-R03 | 18/10/2019 |
| 5 | 110kV AIS Station Typical Control Room Layout | XDN-CR-STND-H-001-R01 | 18/10/2019 |
| 6 | 110/220/400kV Station General Requirements | XDS-GFS-00-001-R4 | 19/12/2019 |

It should be noted that requirements can change based on new technologies, safe working standards or lessons learned during construction, operation and decommissioning.

There are a wide variety of potential transmission connection solutions. The layouts provided here are concept designs of the most commonly acceptable solutions and are provided for guidance only.

AIS substations are open-terminal air –insulated, whereas GIS substations are metal enclosed gas-insulated. GIS substations are located indoors and AIS substation are generally located outdoors.

Detailed project specific documentation is provided to applicants who have executed a connection offer with EirGrid.

EirGrid will work with Customers and provided technical assistance with their planning drawings to incorporate technical feedback in advance of finalising their planning submissions.

Customers are encouraged to check that they are using the most up to date information.

For further information on the connection offer process please refer: [**http://www.eirgridgroup.com/customer-and-industry/becoming-a-customer/**](http://www.eirgridgroup.com/customer-and-industry/becoming-a-customer/)

For customers currently engaging with EirGrid in the connection offer process, further detailed specifications and standards can be made available on the EirGrid Extranet page. (Requests for access to the EirGrid extranet page for Transmission standards should be submitted to [info@eirgrid.com](mailto:info@eirgrid.com).)

Information provided to Customers on this website contains general and technical information, which is subject to change from time to time without notice. EirGrid makes no warranties or representations of any kind with respect to the general and technical information provided or the content of any other document or website referred to on this website. EirGrid cannot determine any proposed connection methods until the formal connection application process is completed. Until an application is submitted and the relevant detailed studies and an executed connection agreement is complete, EirGrid will not be in a position to confirm specific technical details. Customers should not act or refrain from acting on the basis of any information provided without seeking appropriate professional advice.

Use of the information provided is solely at the User's own risk. EirGrid does not accept liability for any loss or damage arising from use or reliance on the information provided.